VXI Test Head Fixturing Software Version 3.1

74LS165

74LS165

ls165.vxi Thu Mar 27 12:04:43 1997

Wilson Li

8-Bit Parallel-to-Serial Shift Register

VXI Test Head Fixturing Software Version 3.1 ls165.vxi: 2 of 8

       Module 0

Pod  0:   A Outside  Left
Timing Pod  0/01 [Timing]

            Port 0
  7: N/C          Unused Control 7
  6: N/C          Unused Control 6
  5: N/C          Unused Control 5
  4: N/C          Unused Control 4
  3: N/C          Unused Control 3
  2: N/C          Unused Control 2
  1: Output       CP2
  0: Output       CP1
RDY: N/C          External Signal!
TRG: N/C          External Signal!

            Port 1
  9: N/C          Unused Q 9
  8: N/C          Unused Q 8
  7: N/C          Unused Q 7
  6: N/C          Unused Q 6
  5: N/C          Unused Q 5
  4: N/C          Unused Q 4
  3: N/C          Unused Q 3
  2: N/C          Unused Q 2
  1: N/C          External Signal!
  0: N/C          External Signal!

                                     Module 1

                                   Pod  1:   D     N/C   N/C
                                  Data Pod  1/01 [Pattern I/O]

                                                      Port 0
                                                 0: N/C          Unused Pin   1
                                                 1: N/C          Unused Pin   2
                                                 2: N/C          Unused Pin   3
                                                 3: N/C          Unused Pin   4
                                                 4: N/C          Unused Pin   5
                                                 5: N/C          Unused Pin   6
                                                 6: N/C          Unused Pin   7
                                                 7: N/C          Unused Pin   8
                                               ~OE: N/C          External Signal!
                                               CLK: N/C          External Signal!

                                                      Port 1
                                                 0: N/C          Unused Pin   9
                                                 1: N/C          Unused Pin  10
                                                 2: N/C          Unused Pin  11
                                                 3: N/C          Unused Pin  12
                                                 4: N/C          Unused Pin  13
                                                 5: N/C          Unused Pin  14
                                                 6: N/C          Unused Pin  15
                                                 7: N/C          Unused Pin  16
                                               ~OE: N/C          External Signal!
                                               CLK: N/C          External Signal!

                                   Pod  2:   D     N/C   N/C
                                  Data Pod  2/23 [Pattern I/O]

                                                      Port 2
                                                 0: N/C          Unused Pin  17
                                                 1: N/C          Unused Pin  18
                                                 2: N/C          Unused Pin  19
                                                 3: N/C          Unused Pin  20
                                                 4: N/C          Unused Pin  21
                                                 5: N/C          Unused Pin  22
                                                 6: N/C          Unused Pin  23
                                                 7: N/C          Unused Pin  24
                                               ~OE: N/C          External Signal!
                                               CLK: N/C          External Signal!

                                                      Port 3
                                                 0: N/C          Unused Pin  25
                                                 1: N/C          Unused Pin  26
                                                 2: N/C          Unused Pin  27
                                                 3: N/C          Unused Pin  28
                                                 4: N/C          Unused Pin  29
                                                 5: N/C          Unused Pin  30
                                                 6: N/C          Unused Pin  31
                                                 7: N/C          Unused Pin  32
                                               ~OE: N/C          External Signal!
                                               CLK: N/C          External Signal!

                                                                   Module 2

                                                                      Pod  3:   C Outside  Left
                                                                     Data Pod  3/01 [Pattern I/O]

                                                                                                Port 0
                                                                                               0: Output       P<0>
                                                                                               1: Output       P<1>
                                                                                               2: Output       P<2>
                                                                                               3: Output       P<3>
                                                                                               4: Output       P<4>
                                                                                               5: Output       P<5>
                                                                                               6: Output       P<6>
                                                                                               7: Output       P<7>
                                                                                             ~OE: N/C          External Signal!
                                                                                             CLK: N/C          External Signal!

                                                                                                Port 1
                                                                                               0: Input        Q<7>_Bar
                                                                                               1: Input        Q<7>
                                                                                               2: N/C          Unused Pin  43
                                                                                               3: N/C          Unused Pin  44
                                                                                               4: N/C          Unused Pin  45
                                                                                               5: N/C          Unused Pin  46
                                                                                               6: N/C          Unused Pin  47
                                                                                               7: N/C          Unused Pin  48
                                                                                             ~OE: N/C          External Signal!
                                                                                             CLK: N/C          External Signal!

                                                                      Pod  4:   C Outside Right
                                                                     Data Pod  4/23 [Pattern I/O]

                                                                                                Port 2
                                                                                               0: Output       PL
                                                                                               1: Output       DS
                                                                                               2: N/C          Unused Pin  51
                                                                                               3: N/C          Unused Pin  52
                                                                                               4: N/C          Unused Pin  53
                                                                                               5: N/C          Unused Pin  54
                                                                                               6: N/C          Unused Pin  55
                                                                                               7: N/C          Unused Pin  56
                                                                                             ~OE: N/C          External Signal!
                                                                                             CLK: N/C          External Signal!

                                                                                                Port 3
                                                                                               0: N/C          Unused Pin  57
                                                                                               1: N/C          Unused Pin  58
                                                                                               2: N/C          Unused Pin  59
                                                                                               3: N/C          Unused Pin  60
                                                                                               4: N/C          Unused Pin  61
                                                                                               5: N/C          Unused Pin  62
                                                                                               6: N/C          Unused Pin  63
                                                                                               7: N/C          Unused Pin  64
                                                                                             ~OE: N/C          External Signal!
                                                                                             CLK: N/C          External Signal!

VXI Test Head Fixturing Software Version 3.1 ls165.vxi: 3 of 8

 IC Signal Name      IWA OWA POD_##

  1 PL                00 128 2:0  4
  2 CP1               01  39 0:0  0
  3 P<4>              02 164 0:4  3
  4 P<5>              03 165 0:5  3
  5 P<6>              04 166 0:6  3
  6 P<7>              05 167 0:7  3
  7 Q<7>_Bar          06 176 1:0  3
  8 GND               07
  9 Q<7>              37 177 1:1  3
 10 DS                36 129 2:1  4
 11 P<0>              35 160 0:0  3
 12 P<1>              34 161 0:1  3
 13 P<2>              33 162 0:2  3
 14 P<3>              32 163 0:3  3
 15 CP2               31  38 0:1  0
 16 VCC               30

 IC Signal Name      IWA OWA POD_##

VXI Test Head Fixturing Software Version 3.1 ls165.vxi: 4 of 8

Connector - Pod View

VXI Test Head Fixturing Software Version 3.1 ls165.vxi: 5 of 8

Inner Wiring Array - Outer Wiring Array View

VXI Test Head Fixturing Software Version 3.1 ls165.vxi: 6 of 8

Inner Wiring Array Reference View (Colour)

VXI Test Head Fixturing Software Version 3.1 ls165.vxi: 7 of 8

Inner Wiring Array Reference View (B&W)

VXI Test Head Fixturing Software Version 3.1 ls165.vxi: 8 of 8

IC - PGA Socket View